Devices and Modules: Other Devices

All images on this page are thumbnails on which you can click to bring up a larger image.

Hub-PT

The Hub-PT provides ten slots.

Module Name | Thumbnail | Description
PT-REPEATER-NM-1CE |  | The PT-REPEATER-NM-1CE features a single Ethernet port that can connect a LAN backbone which can also support either six PRI connections to aggregate ISDN lines, or 24 synchronous/asynchronous ports.
PT-REPEATER-NM-1CFE |  | The PT-REPEATER-NM-1CFE Module provides 1 Fast-Ethernet interface for use with copper media. Ideal for a wide range of LAN applications, the Fast Ethernet network modules support many internetworking features and standards. Single port network modules offer autosensing 10/100BaseTX or 100BaseFX Ethernet. The TX (copper) version supports virtual LAN (VLAN) deployment.
PT-REPEATER-NM-1CGE |  | The single-port Cisco Gigabit Ethernet Network Module (part number PT-REPEATER-NM-1CGE) provides Gigabit Ethernet copper connectivity for access routers. The module is supported by the Cisco 2691, Cisco 3660, Cisco 3725, and Cisco 3745 series routers. This network module has one gigabit interface converter (GBIC) slot to carry any standard copper or optical Cisco GBIC.
PT-REPEATER-NM-1FFE |  | The PT-REPEATER-NM-1FFE Module provides 1 Fast-Ethernet interface for use with fiber media. Ideal for a wide range of LAN applications, the Fast Ethernet network modules support many internetworking features and standards. Single port network modules offer autosensing 10/100BaseTX or 100BaseFX Ethernet.
PT-REPEATER-NM-1FGE |  | The single-port Cisco Gigabit Ethernet Network Module (part number PT-REPEATER-NM-1FGE) provides Gigabit Ethernet optical connectivity for access routers. The module is supported by the Cisco 2691, Cisco 3660, Cisco 3725, and Cisco 3745 series routers. This network module has one gigabit interface converter (GBIC) slot to carry any standard copper or optical Cisco GBIC.

Repeater-PT

The Repeater-PT provides two slots.

The Repeater-PT supports the same modules that the Hub-PT supports.

AccessPoint-PT

The AccessPoint-PT has a built-in antenna and provides one slot.

The AccessPoint-PT supports the same modules that the Hub-PT supports.

Linksys-WRT300N

The Linksys-WRT300N wireless router has a built-in antenna and provides four fixed 10/100 (100BASE-TX) Ethernet ports and one fixed Internet port (also 100BASE-TX, typically for connection to cable and DSL modems).

The Linksys-WRT300N wireless router does not support modules.

Cloud-PT

Although a cloud is not a single device, Packet Tracer 5.0 gives you access to a representation of a cloud. It provides ten slots, a console port, and an auxiliary port.

Device Name | Thumbnail | Description
PT-CLOUD-NM-1AM |  | The PT-CLOUD-NM-1AM card features dual RJ-11 connectors, which are used for basic telephone service connection. The WIC-1AM uses one port for connection to a standard telephone line, and the other port can be connected to a basic analog telephone for use when the modem is idle.
PT-CLOUD-NM-1CE |  | The PT-CLOUD-NM-1CE features a single Ethernet port that can connect a LAN backbone which can also support either six PRI connections to aggregate ISDN lines, or 24 synchronous/asynchronous ports.
PT-CLOUD-NM-1CX |  | The PT-CLOUD-NM-1CX card features a single coaxial connector, which are used for cable modem service connection.
PT-CLOUD-NM-1S |  | The PT-CLOUD-NM-1S provides a single port serial connection to remote sites or legacy serial network devices such as Synchronous Data Link Control (SDLC) concentrators, alarm systems, and packet over SONET (POS) devices.

DSL-Modem-PT

The DSL-Modem-PT provides one slot.

Device Name | Thumbnail | Description
PT-MODEM-NM-1CE |  | The PT-MODEM-NM-1CE features a single Ethernet port that can connect a LAN backbone which can also support either six PRI connections to aggregate ISDN lines, or 24 synchronous/asynchronous ports.
PT-MODEM-NM-1CFE |  | The PT-MODEM-NM-1CFE Module provides 1 Fast-Ethernet interface for use with copper media. Ideal for a wide range of LAN applications, the Fast Ethernet network modules support many internetworking features and standards. Single port network modules offer autosensing 10/100BaseTX or 100BaseFX Ethernet. The TX (copper) version supports virtual LAN (VLAN) deployment.
PT-MODEM-NM-1CGE |  | The single-port Cisco Gigabit Ethernet Network Module (part number PT-MODEM-NM-1CGE) provides Gigabit Ethernet copper connectivity for access routers. The module is supported by the Cisco 2691, Cisco 3660, Cisco 3725, and Cisco 3745 series routers. This network module has one gigabit interface converter (GBIC) slot to carry any standard copper or optical Cisco GBIC.

Cable-Modem-PT

The Cable-Modem-PT provides one slot.

The Cable-Modem-PT supports the same modules that the DSL-Modem-PT supports.